监听程序接口文档

**仪器：**

SA7000

**图片：**

**配置：**

[{"MachID":"#RowID","Type":"DataBase","UpTime":"20000","Address":"DSN=Sa7000\_2002","UpCDF":"","UpREF":"","DealProcess":"MI.MIFSA7000","Para":"SELECT 日期,序号,血浆粘度,压积,全血高切相对指数,全血低切相对指数,红细胞聚集指数,全血高切还原粘度,全血低切还原粘度,红细胞变形指数TK,红细胞刚性指数,ShearRate,Visc FROM TestData,Visc WHERE TestData.TestDataID=Visc.TestDataID AND \"日期\"=date()","PreDealClass":"PreDeal.DealDemo,PreDeal","UPPreDealClass":""}]

**M:**

Class MI.MIFSA7000 Extends %Persistent  
{  
  
ClassMethod fileMTHD(mi, record, epis, P3, P4, P5, P6, P7, P8, P9, P10, P11, P12, P13, Sessions, Output RowCount As %String) As %String  
{  
    s mi=$g(mi)  
    i '$d(^dbo.BTMIMachineParameterD(mi)) q  
    i '$l(record) q  
    s a=$p($h,",",1)  
    s b=$zdh($p(record,"~",1),8)  
    i b=a  d  
    .;d Trace^MI.MIF000(mi,record,"H<--M")  
    .s (sample,epis,result,date,time,QC)=""  
    .s record=$tr(record,"~","|")  
    .;d Trace^MI.MIF000(mi,record,"H<--M")  
   .s CODE="XJND^HCT^gqxd^dqxd^HJJ^dqhy^gqhy^htk^HGX"  
   .s epis=$p(record,"|",2)  
   .s k=$l(record,"|")-2  
   .f i=3:1:k d   
   ..i i=k  d  
   ...s code=$p(record,"|",k)  
   ...s res=$p(record,"|",k+1)  
   ...s result=result\_code\_$c(92)\_res\_$c(44)  
   ..e  d  
   ...s code=$P(CODE,"^",i-2)  
   ...s res=$p(record,"|",i)  
   ...;s ^TMP("0720",$h)=res  
   ...s result=result\_code\_$c(92)\_res\_$c(44)  
   .i ($g(^TMP("SA7000",$p($h,",",1),epis,result))'=1)||('$d(^TMP("SA7000",$p($h,",",1),epis,result))) d  
   ..d Trace^MI.MIF000(mi,record,"H<--M")  
   ..i epis="QC" d  
   ...s code=code-8  
   ..i $l(epis),$l(result) d ##Class(MI.Common.MIFBase).Save(mi, epis, result, date, time, QC)  
   ..s ^TMP("SA7000",$p($h,",",1),epis,result)=1  
    q ""  
}  
  
}