监听程序接口文档

**仪器：**

YHLO

**图片：**

**配置：** [{"MachID":"#RowID","Type":"Drect","UpTime":"3000","Address":"C:\\Users\\le\\AppData\\Roaming\\Union\\Host","UpCDF":"","UpREF":"","DealProcess":"MI.MIFYELO","Para":".xml","PreDealClass":"PreDeal.DealDemo,PreDeal","UPPreDealClass":""}]

**M:**

Class MI.MIFYELO Extends %Persistent  
{  
  
ClassMethod fileMTHD(mi, record, epis, P3, P4, P5, P6, P7, P8, P9, P10, P11, P12, P13, Sessions, Output RowCount As %String) As %String  
{  
 s mi=$g(mi)  
   i '$d(^dbo.BTMIMachineParameterD(mi)) q  
 i '$l(record) q  
 s record=$tr(record,"</>")  
 i $l(record) d  
 .i record["?" q  
 .i record["Results" q  
  .s (sample,epis,result,date,time,QC)=""  
  .s record=$p(record," ",4,$l(record," "))  
  .s record=$tr(record," ","|")  
  .d Trace^MI.MIF000(mi,record,"H<--M")  
  .s episcode=$p($p(record,"|",1),"=",2)  
  .s epis=$e(episcode,2,$l(episcode)-1)  
  .s reccode=$p($p(record,"|",2),"=",2)  
  .s code=$e(reccode,2,$l(reccode)-1)  
  .s rescode=$p($p(record,"|",8),"=",2)  
  .s res=$e(rescode,2,$l(rescode)-1)  
    .i $l(res) s result=result\_code\_$c(92)\_res\_$c(44)  
 i $l(epis),$l(result) d ##Class(MI.Common.MIFBase).Save(mi, epis, result, date, time, QC)  
    i $l(epis) s retVal=$$ReceiveLabno^MI.MIF000(mi,epis,"")  
 q ""  
}  
  
}