监听程序接口文档

**仪器：**

F60

**图片：**

**配置：**

[{"MachID":"#RowID","Type":"DataBase","UpTime":"3000","Address":"DSN=F1601","UpCDF":"","UpREF":"","DealProcess":"MI.MIFF160","Para":"SELECT \* FROM report where \"yisheng\" Not Like '1' #yisheng# UPDATE report set \"yisheng\" = '1' where \"yisheng\" Not Like '1' ","PreDealClass":"PreDeal.DealDemo,PreDeal","UPPreDealClass":""}]

**M:**

Class MI.MIFF160 Extends %Persistent  
{  
  
ClassMethod fileMTHD(mi, record, epis, P3, P4, P5, P6, P7, P8, P9, P10, P11, P12, P13, Sessions, Output RowCount As %String) As %String  
{  
 s mi=$g(mi)  
   i '$d(^dbo.BTMIMachineParameterD(mi)) q  
 i '$l(record) q  
 i $l(record) d  
  .;d Trace^MI.MIF000(mi,record,"H<--M")  
  .s (sample,epis,result,date,time,QC)=""  
  .s record=$tr(record,"~","|")  
  .d Trace^MI.MIF000(mi,record,"H<--M")  
    .s CODE="bianhao,weizhi,xingming,xingbie,nianling,zhonglei,yisheng,XWJxiangpianshu,lujing,shijiban,wancheng,chongce,binglihao,laiyuan,keshi,bingqu,chuanghao,fenbianyanse,xingzhuang,hongxibao,baixibao,shiwuxibao,buxiaohuashiwu,gouchongluan,yuanchong,baonang,huichongluan,meijunbaozi,qita,bianchongluan,jushixibao,yinxiehuaxue,qitachongluan,jiadishi,yinxiemianyi,changdichong,xialeidengshi,xianbingdu,lunzhuanbingdu,kesaqi,youmenluoxuan,jianyanyisheng,shenheyisheng,baogaoriqi,beizhu,zongbianhao,zhifangqiu,songjianriqi,linchuangzhenduan,riqi,jianyanxuanxiang,dangqianzhaopian,tianjiariqi"  
    .s epis=$p(record,"|",1)  
    .s k=$l(record,"|")-6  
    .f i=17:1:k d   
    ..s code=$P(CODE,",",i)  
    ..s res=$p(record,"|",i)  
    ..i $l(res) s result=result\_code\_$c(92)\_res\_$c(44)  
 .i $l(epis),$l(result) d ##Class(MI.Common.MIFBase).Save(mi, epis, result, date, time, QC)  
    .i $l(epis) s retVal=$$ReceiveLabno^MI.MIF000(mi,epis,"")  
 q ""  
}  
  
}